Using the µVision Socket Interface: Powerscale Functions

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
Powerscale Functions
Client Functions

## Functions
_UVSC_FUNC_ UVSC_STATUS | UVSC_POWERSCALE_SHOWCODE (int iConnHandle, UVSC_PSTAMP *pPowerScaleData)

## Description

## Function Documentation

_UVSC_FUNC_ UVSC_STATUS UVSC_POWERSCALE_SHOWCODE | ( | int | iConnHandle,
|  | UVSC_PSTAMP * | pPowerScaleData
| ) |  |

Show code at a specific time stamp within uVision

Parameters

  iConnHandle | Handle for the connection, as returned by UVSC_OpenConnection
  pPowerScaleData | Pointer to a UVSC_PSTAMP structure containing the time stamp to show code and trace

Returns
  UVSC_STATUS_SUCCESS on success, or an error code

Precondition
  UVSC_OpenConnection must have been called successfully
  uVision is in debug mode

Use this function to show code at a specific time stamp within uVision. The time stamp consists of ticks since reset and time since last tick.