Using the µVision Socket Interface: UV_MRANGE Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
UV_MRANGE Struct Reference
Structs

## Data Fields
DWORD | mType: 8
| Memory type (UV_MR_NONE / UV_MR_ROM / UV_MR_RAM) More...
DWORD | dfltRam: 1
| 1:=default RAM range More...
DWORD | dfltRom: 1
| 1:=default ROM range More...
DWORD | isZiRam: 1
| 1:=RAM range zero-initialized More...
DWORD | __pad0__:21
| Reserved. More...
DWORD | nRes [3]
| Reserved. More...
xU64 | nStart
| Memory range start address. More...
xU64 | nSize
| Memory range size. More...

## Description

Individual memory range data

Indicates how a memory range is configured.

This is a sub-structure and is not contained in any message directly.

## Field Documentation

DWORD UV_MRANGE::__pad0__

Reserved.

DWORD UV_MRANGE::dfltRam

1:=default RAM range

DWORD UV_MRANGE::dfltRom

1:=default ROM range

DWORD UV_MRANGE::isZiRam

1:=RAM range zero-initialized

DWORD UV_MRANGE::mType

Memory type (UV_MR_NONE / UV_MR_ROM / UV_MR_RAM)

DWORD UV_MRANGE::nRes[3]

Reserved.

xU64 UV_MRANGE::nSize

Memory range size.

xU64 UV_MRANGE::nStart

Memory range start address.