Using the µVision Socket Interface: Data Fields

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- i
- j
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - b -

- bArray : VARINFO
- bAsm : iSHOWSYNC
- bAsmRes : iSHOWSYNC
- bAuto : VARINFO
- bAutoStart : iINTERVAL
- bChanged : IVARENUM
- bClass : VARINFO
- bCycles : iINTERVAL
- bEcho : EXECCMD
- bEditable : VARINFO
- bEnabled : MENUENUM
- bEnum : VARINFO
- bExtended : iSTKENUM
- bExtendedStack : UVSOCK_OPTIONS
- bFull : ADRMTFL , iPATHREQ , iSTKENUM
- bFunction : VARINFO
- bGlobal : VARINFO
- bHll : iSHOWSYNC
- bHllRes : iSHOWSYNC
- bkchg : UVSOCK_CMD_DATA
- bkparm : UVSOCK_CMD_DATA
- bModified : iSTKENUM
- bName : VARINFO
- bParam : VARINFO
- bPointer : VARINFO
- bQualified : VARINFO
- brk : UVSOCK_CMD_RESPONSE
- bSetInterval : iINTERVAL
- bStatic : VARINFO
- bStruct : VARINFO
- bType : VARINFO
- bUnion : VARINFO
- bValue : AVTR , iVTRENUM , VARINFO