Using the µVision Socket Interface: UVSOCK_OPTIONS Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
UVSOCK_OPTIONS Struct Reference
Structs

## Data Fields
DWORD | bExtendedStack: 1
| Extended stack mode: allows task enumeration, read/write variables and expressions. More...
DWORD | __pad0__:31
| reserved More...

## Description

UVSOCK options

Flags to configure UVSOCK

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_GEN_SET_OPTIONS

## Field Documentation

DWORD UVSOCK_OPTIONS::__pad0__

reserved

DWORD UVSOCK_OPTIONS::bExtendedStack

Extended stack mode: allows task enumeration, read/write variables and expressions.