Using the µVision Socket Interface: Data Structure Index

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structure Index
A | B | C | D | E | I | M | P | R | S | T | U | V

A
D
| IVARENUM | SSTR | UVSOCK_CMD_DATA
M
| STACKENUM | UVSOCK_CMD_RESPONSE
ADRMTFL | DBGTGTOPT |
T
| UVSOCK_ERROR_RESPONSE
AFLMAP | DEC_EVENT | MENUENUM | UVSOCK_OPTIONS
AMEM |
E
| MENUID | TASKENUM |
V
AVTR |
P
| TRNOPT
B
| ENUMTPM | TVAL | VARINFO
EVTR_CMDSTAT | PGRESS |
U
| VARVAL
BKCHG | EVTR_PACK | PRJDATA | VSET
BKPARM | EVTROUT |
R
| UV_MEMINFO |
i
BKRSP | EXECCMD | UV_MRANGE
BPREASON | EXTVERS | RAW_EVENT | UVLICINFO | iINTERVAL
C
I
| REGENUM | UVSC_CB_DATA | iPATHREQ
S
| UVSC_PSTAMP | iSHOWSYNC
CYCTS | ITMOUT | UVSOCK_CMD | iSTKENUM
|  | SERIO |  |

A | B | C | D | E | I | M | P | R | S | T | U | V