Using the µVision Socket Interface: UVSC_CB_DATA Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
UVSC_CB_DATA Struct Reference
Client Structs

## Data Fields
UVSOCK_CMD | msg
| UVSOCK fromatted message (returned when UVSC_CB_TYPE is UVSC_CB_ASYNC_MSG, UVSC_CB_BUILD_OUTPUT_MSG, UVSC_CB_CMD_OUTPUT_MSG or UVSC_CB_PROGRESS_BAR_MSG) More...
UVSC_STATUS | err
| Error notification (returned when UVSC_CB_TYPE is UVSC_CB_ERROR) More...
int | iConnHandle
| UVSC connection handle (returned when UVSC_CB_TYPE is UVSC_CB_DISCONNECTED) More...

## Description

UVSC callback data

Contains the data retuned in the UVSC callback function uvsc_cb configured through UVSC_OpenConnection.

## Field Documentation

UVSC_STATUS UVSC_CB_DATA::err

Error notification (returned when UVSC_CB_TYPE is UVSC_CB_ERROR)

int UVSC_CB_DATA::iConnHandle

UVSC connection handle (returned when UVSC_CB_TYPE is UVSC_CB_DISCONNECTED)

UVSOCK_CMD UVSC_CB_DATA::msg

UVSOCK fromatted message (returned when UVSC_CB_TYPE is UVSC_CB_ASYNC_MSG, UVSC_CB_BUILD_OUTPUT_MSG, UVSC_CB_CMD_OUTPUT_MSG or UVSC_CB_PROGRESS_BAR_MSG)