Using the µVision Socket Interface: iPATHREQ Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
iPATHREQ Struct Reference
Structs

## Data Fields
UINT | bFull: 1
| 1:=want full path(s), 0:=want relative path(s) More...
UINT | __pad0__:31
| Reserved. More...
UINT | nRes [7]
| Reserved. More...

## Description

Path request data structure

Contains data indicating how a path retreival should be performed.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_PRJ_GET_OUTPUTNAME (Set all reserved items to 0)
- UV_PRJ_GET_CUR_TARGET (Set to 0 for now, unused)

## Field Documentation

UINT iPATHREQ::__pad0__

Reserved.

UINT iPATHREQ::bFull

1:=want full path(s), 0:=want relative path(s)

UINT iPATHREQ::nRes[7]

Reserved.