Using the µVision Socket Interface: VARVAL Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
VARVAL Struct Reference
Structs

## Data Fields
IVARENUM | variable
| Variable to set new value. More...
SSTR | value
| Value to set. More...

## Description

Variable set request

Extended stack mode only

Contains data indicating enumeration should be performed.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_VARIABLE_SET ()

## Field Documentation

SSTR VARVAL::value

Value to set.

IVARENUM VARVAL::variable

Variable to set new value.