Using the µVision Socket Interface: EVTR_CMDSTAT Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
EVTR_CMDSTAT Struct Reference

## Data Fields
DWORD | cmdStat
| Command or Status. More...
DWORD | nMany
| number of items (BYTE) More...
char * | data
| reserved More...

## Description

Event Viewer register / unregister

Client ==> uVision (Request)

- UV_DBG_EVTR_REGISTER / UV_DBG_EVTR_UNREGISTER

Client <== uVision (Response)

## Field Documentation

DWORD EVTR_CMDSTAT::cmdStat

Command or Status.

char* EVTR_CMDSTAT::data

reserved

DWORD EVTR_CMDSTAT::nMany

number of items (BYTE)