Using the µVision Socket Interface: Build Return Codes

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations
Build Return Codes
Enumerations

## Enumerations
enum | UVBUILDCODES { UVBUILD_OK = 1, UVBUILD_OK_WARNINGS = 2, UVBUILD_ERRORS = 3, UVBUILD_CANCELLED = 4, UVBUILD_CLEANED = 5, UVBUILD_CODES_END }

## Description

## Enumeration Type Documentation

enum UVBUILDCODES

Build Completion Codes

The build completetion codes indicate the completion status of a uVision build.

Enumerator
UVBUILD_OK | Build was Ok - no errors and warnings.
UVBUILD_OK_WARNINGS | Build was Ok - with warnings.
UVBUILD_ERRORS | Build failed - with error(s)
UVBUILD_CANCELLED | Build was stopped/cancelled.
UVBUILD_CLEANED | Project clean was completed.
UVBUILD_CODES_END | Always at end.