Using the µVision Socket Interface: DEC_EVENT Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
DEC_EVENT Struct Reference

## Data Fields
UINT32 | nType: 8
UINT32 | nRes: 24
UINT64 | EvNumber
UINT64 | tStamp
char | szText [1]

## Field Documentation

UINT64 DEC_EVENT::EvNumber

UINT32 DEC_EVENT::nRes

UINT32 DEC_EVENT::nType

char DEC_EVENT::szText[1]

UINT64 DEC_EVENT::tStamp