Using the µVision Socket Interface: ADRMTFL Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
ADRMTFL Struct Reference
Structs

## Data Fields
UINT | bFull: 1
| 1:=want full path, 0:=want relative path More...
UINT | __pad0__: 31
| Reserved. More...
xU64 | nAdr
| Address to map. More...
UINT | nRes [7]
| Reserved. More...

## Description

Map address to file / line request data

Contains request information for mapping a code address to a file and line number.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_ADR_TOFILELINE (Set bFull to 1 to retrieve the file as an absolute path, or 0 to retrieve as a relative path, and set nAdr to the address to map)

## Field Documentation

UINT ADRMTFL::__pad0__

Reserved.

UINT ADRMTFL::bFull

1:=want full path, 0:=want relative path

xU64 ADRMTFL::nAdr

Address to map.

UINT ADRMTFL::nRes[7]

Reserved.