Using the µVision Socket Interface: UV_MEMINFO Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
UV_MEMINFO Struct Reference
Structs

## Data Fields
UINT | nRanges
| Number of UV_MRANGE memory ranges pointed to by &mr. More...
UINT | nRes [8]
| Reserved. More...
UV_MRANGE | mr
| Zero or more memory ranges. More...

## Description

Memory ranges data

List of memory ranges set within the uVision project.

This structure is used in the following messages:

Client <== uVision (Response)

- UV_PRJ_GET_OPTITEM (uVision sets 'Item data string' of the TRNOPT structure to UV_MEMINFO. Within UV_MEMINFO uVision sets nRanges to the number of memory ranges and mr to the actual memory ranges data)

## Field Documentation

UV_MRANGE UV_MEMINFO::mr

Zero or more memory ranges.

UINT UV_MEMINFO::nRanges

Number of UV_MRANGE memory ranges pointed to by &mr.

UINT UV_MEMINFO::nRes[8]

Reserved.