Using the µVision Socket Interface: UVLICINFO Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
UVLICINFO Struct Reference
Structs

## Data Fields
DWORD | rvmdk: 1
| 1:=RV-MDK is licensed, 0:=RV-MDK is not licensed More...
DWORD | __pad0__: 31
| Reserved. More...
DWORD | nRes [10]
| Reserved. More...

## Description

Licensing data

Indicates which uVision modules are licensed. Currently implemented for ARM RealView MDK only.

This structure is used in the following messages:

Client <== uVision (Response)

- UV_GEN_CHECK_LICENSE (uVision sets rvmdk)

## Field Documentation

DWORD UVLICINFO::__pad0__

Reserved.

DWORD UVLICINFO::nRes[10]

Reserved.

DWORD UVLICINFO::rvmdk

1:=RV-MDK is licensed, 0:=RV-MDK is not licensed