Using the µVision Socket Interface: UVSOCK_ERROR_RESPONSE Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
UVSOCK_ERROR_RESPONSE Struct Reference
Structs

## Data Fields
UINT | nRes1
| Reserved. More...
UINT | nRes2
| Reserved. More...
UINT | StrLen
| Length of error string (including terminator) in bytes. More...
BYTE | str [SOCK_NDATA-20]
| Error description. More...

## Description

Error response data

Contains error information. The union in UVSOCK_CMD_RESPONSE will correspond to this structure if the status code within is anything other than UV_STATUS_SUCCESS or if within a UV_ASYNC_MSG.

Contained in UVSOCK_CMD_RESPONSE if an error occurred.

## Field Documentation

UINT UVSOCK_ERROR_RESPONSE::nRes1

Reserved.

UINT UVSOCK_ERROR_RESPONSE::nRes2

Reserved.

BYTE UVSOCK_ERROR_RESPONSE::str[SOCK_NDATA-20]

Error description.

UINT UVSOCK_ERROR_RESPONSE::StrLen

Length of error string (including terminator) in bytes.