Using the µVision Socket Interface: DBGTGTOPT Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
DBGTGTOPT Struct Reference
Structs

## Data Fields
DWORD | target: 1
| Target type (UV_TARGET_HW:=Target is hardware, UV_TARGET_SIM:=Target is simulator) More...
DWORD | __pad0__: 31
| Reserved. More...
DWORD | nRes [10]
| Reserved. More...

## Description

Target debugging data

Indicates how the target will be debugged when debug mode is entered.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_PRJ_SET_DEBUG_TARGET (Set target to the type of debugging to perform)

Client <== uVision (Response)

- UV_PRJ_GET_DEBUG_TARGET (uVision sets target to the type of debugging that will be performed)

## Field Documentation

DWORD DBGTGTOPT::__pad0__

Reserved.

DWORD DBGTGTOPT::nRes[10]

Reserved.

DWORD DBGTGTOPT::target

Target type (UV_TARGET_HW:=Target is hardware, UV_TARGET_SIM:=Target is simulator)