Using the µVision Socket Interface: iSTKENUM Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
iSTKENUM Struct Reference
Structs

## Data Fields
UINT | bFull: 1
| Unused, kept for backward compatibility. More...
UINT | bExtended: 1
| Get extended information: nVars, nTotal, iTask (see STACKENUM) Extended stack mode only More...
UINT | bModified: 1
| Enumerate only modified frames Extended stack mode only More...
UINT | __pad0__:29
| Reserved. More...
UINT | nTask
| Task ID: reserved for RTX case, otherwise ignored. More...
UINT | nRes [6]
| Reserved. More...

## Description

Stack enumeration request data

Contains data indicating how a stack enumeration should be performed.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_ENUM_STACK (Set all items to 0)

## Field Documentation

UINT iSTKENUM::__pad0__

Reserved.

UINT iSTKENUM::bExtended

Get extended information: nVars, nTotal, iTask (see STACKENUM) Extended stack mode only

UINT iSTKENUM::bFull

Unused, kept for backward compatibility.

UINT iSTKENUM::bModified

Enumerate only modified frames Extended stack mode only

UINT iSTKENUM::nRes[6]

Reserved.

UINT iSTKENUM::nTask

Task ID: reserved for RTX case, otherwise ignored.