Using the µVision Socket Interface: EXECCMD Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
EXECCMD Struct Reference
Structs

## Data Fields
UINT | bEcho: 1
| 1:=echo command and response in uVision Command Window, 0:=no echo More...
UINT | __pad0__:31
| Reserved. More...
UINT | nRes [7]
| Reserved. More...
SSTR | sCmd
| Command to execute. More...

## Description

Command execution request / response data

Contains data indicating how and which command uVision should execute.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_EXEC_CMD (Set bEcho to 1 to echo the command and result in the uVision Command Window, or 0 for no echo. Set sCmd to the command string to execute)

## Field Documentation

UINT EXECCMD::__pad0__

Reserved.

UINT EXECCMD::bEcho

1:=echo command and response in uVision Command Window, 0:=no echo

UINT EXECCMD::nRes[7]

Reserved.

SSTR EXECCMD::sCmd

Command to execute.