Using the µVision Socket Interface: BKCHG Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
BKCHG Struct Reference
Structs

## Data Fields
CHG_TYPE | type
| Type of operation to perform on the breakpoint. More...
UINT | nTickMark
| Timestamp of breakpoint as returned by UV_DBG_ENUMERATE_BP. More...
UINT | nRes [8]
| Reserved (set to 0) More...

## Description

Breakpoint change data

Data indentifying an operation to be applied to an individual breakpoint.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_CHANGE_BP (Set type to the operation to perform and set nTickMark to the value returned by the UV_DBG_ENUMERATE_BP command)

## Field Documentation

UINT BKCHG::nRes[8]

Reserved (set to 0)

UINT BKCHG::nTickMark

Timestamp of breakpoint as returned by UV_DBG_ENUMERATE_BP.

CHG_TYPE BKCHG::type

Type of operation to perform on the breakpoint.