Using the µVision Socket Interface: iVTRENUM Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
iVTRENUM Struct Reference
Structs

## Data Fields
UINT | bValue: 1
| Retreive VTR value. More...
UINT | __pad0__:31
| Reserved. More...
UINT | nRes [7]
| Reserved. More...

## Description

Virtual register (VTR) enumeration request data

Contains data indicating how a VTR enumeration should be performed.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_ENUM_VTR (Set bValue to 1 to retreive the VTR values as well as the list of VTRs)

## Field Documentation

UINT iVTRENUM::__pad0__

Reserved.

UINT iVTRENUM::bValue

Retreive VTR value.

UINT iVTRENUM::nRes[7]

Reserved.