Using the µVision Socket Interface: iSHOWSYNC Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
iSHOWSYNC Struct Reference
Structs

## Data Fields
xU64 | nAdr
| Address of code to show. More...
UINT | bAsm: 1
| 1:=show disassembly More...
UINT | bHll: 1
| 2:=show high level language code More...
UINT | bAsmRes: 1
| Unused. More...
UINT | bHllRes: 1
| Unused. More...
UINT | __pad0__:28
| Reserved. More...
UINT | nRes [7]
| Reserved. More...

## Description

Show code in uVision request data

Contains data indicating how uVision should display code for the requested address.

This structure is used in the following messages:

Client ==> uVision (Request)

- UV_DBG_ADR_SHOWCODE (Set nAdr to the address to show code for, bAsm to 1 to display the assembly code, and bHll to show the high level language code (if possible))

## Field Documentation

UINT iSHOWSYNC::__pad0__

Reserved.

UINT iSHOWSYNC::bAsm

1:=show disassembly

UINT iSHOWSYNC::bAsmRes

Unused.

UINT iSHOWSYNC::bHll

2:=show high level language code

UINT iSHOWSYNC::bHllRes

Unused.

xU64 iSHOWSYNC::nAdr

Address of code to show.

UINT iSHOWSYNC::nRes[7]

Reserved.