Using the µVision Socket Interface: CYCTS Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
CYCTS Struct Reference
Structs

## Data Fields
xU64 | cycles
| Execution time in cycles. More...
double | tStamp
| Execution time in seconds. More...

## Description

Cycles and Time data

Represents the execution time of a simulated target.

This structure is used in the following messages:

Client <== uVision (Response)

- UV_DBG_TIME_INFO (All members are written by uVision)

## Field Documentation

xU64 CYCTS::cycles

Execution time in cycles.

double CYCTS::tStamp

Execution time in seconds.