Using the µVision Socket Interface: REGENUM Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
REGENUM Struct Reference
Structs

## Data Fields
xWORD16 | nGi
xWORD16 | nItem
char | szReg [16]
xUC8 | isPC: 1
xUC8 | canChg: 1
xUC8 | __pad0__: 6
char | szVal [32]

## Description

Register enumeration return data

Contains a register enumeration item.

This structure is used in the following messages:

Client <== uVision (Async)

- UV_DBG_ENUM_REGISTERS_ENU (uVision writes all values)

## Field Documentation

xUC8 REGENUM::__pad0__

xUC8 REGENUM::canChg

xUC8 REGENUM::isPC

xWORD16 REGENUM::nGi

xWORD16 REGENUM::nItem

char REGENUM::szReg[16]

char REGENUM::szVal[32]