Using the µVision Socket Interface: µVision Menu Codes

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations
µVision Menu Codes
Enumerations

## Enumerations
enum | UVMENUTYPES { UVMENU_DEBUG = 0, UVMENU_SYS_VIEW = 1, UVMENU_PERI = 2, UVMENU_RTX = 3, UVMENU_CAN = 4, UVMENU_AGDI = 5, UVMENU_TOOLBOX = 6, UVMENU_END }

## Description

## Enumeration Type Documentation

enum UVMENUTYPES

View types

View types used by menuenum_t structure

Enumerator
UVMENU_DEBUG | Static uVision debug views (Disassembly, ToolBox, Trace Data, etc.)
UVMENU_SYS_VIEW | System viewer views.
UVMENU_PERI | Peripheral dialogs.
UVMENU_RTX | Rtx dialogs (reserved)
UVMENU_CAN | CAN dialogs (reserved)
UVMENU_AGDI | AGDI Extention dialogs (reserved)
UVMENU_TOOLBOX | ToolBox entries.
UVMENU_END | Always at end.