Using the µVision Socket Interface: Data Fields - Variables

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- _
- a
- b
- c
- d
- e
- f
- i
- j
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - c -

- canChg : REGENUM
- cmd : UVSOCK_CMD_RESPONSE
- cmdRsp : UVSOCK_CMD_DATA
- cmdStat : EVTR_CMDSTAT
- complete : RAW_EVENT
- count : BKPARM , BKRSP , IVARENUM , VARINFO
- ctx : RAW_EVENT
- cycles : CYCTS , UVSOCK_CMD