Using the µVision Socket Interface: Breakpoint Type Codes

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations
Breakpoint Type Codes
Enumerations

## Enumerations
enum | BKTYPE { BRKTYPE_EXEC = 1, BRKTYPE_READ = 2, BRKTYPE_WRITE = 3, BRKTYPE_READWRITE = 4, BRKTYPE_COMPLEX = 5, BRKTYPE_END }

## Description

## Enumeration Type Documentation

enum BKTYPE

Breakpoint type definition

Defines the possible types of breakpoints in uVision.

Enumerator
BRKTYPE_EXEC | Execution Breakpoint.
BRKTYPE_READ | Read Access Breakpoint.
BRKTYPE_WRITE | Write Access Breakpoint.
BRKTYPE_READWRITE | ReadWrite Access Breakpoint.
BRKTYPE_COMPLEX | Complex Breakpoint (Expression Breakpoint)
BRKTYPE_END | Always at end.