Using the µVision Socket Interface: Breakpoint Change Codes

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations
Breakpoint Change Codes
Enumerations

## Enumerations
enum | CHG_TYPE { CHG_KILLBP = 1, CHG_ENABLEBP = 2, CHG_DISABLEBP = 3, CHG_END }

## Description

## Enumeration Type Documentation

enum CHG_TYPE

Breakpoint change operation definition

Indicates the type of change to make to a breakpoint in the BKCHG structure

Enumerator
CHG_KILLBP | Delete breakpoint.
CHG_ENABLEBP | Enable breakpoint.
CHG_DISABLEBP | Disable breakpoint.
CHG_END | Always at end.