Using the µVision Socket Interface: AFLMAP Struct Reference

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
AFLMAP Struct Reference
Structs

## Data Fields
UINT | nLine
| Code line number. More...
xU64 | nAdr
| Code address. More...
UINT | iFile
| Index of 'filename' (0 if none) More...
UINT | iFunc
| Index of 'function' (0 if none) More...
int | nRes [5]
| Reserved. More...
char | szFile [1]
| Filename and function (0 [,'filename',0 [,'function',0]]) More...

## Description

Map address to file / line return data

Contains information for a code address to a file and line number mapping.

This structure is used in the following messages:

Client <== uVision (Response)

- UV_DBG_ADR_TOFILELINE (uVision writes nLine to the line number, nAdr to the code address requested, iFile and iFunc to the 'function' and 'filename' indexes within szFile, and szFile to the 'filename' and 'function')

## Field Documentation

UINT AFLMAP::iFile

Index of 'filename' (0 if none)

UINT AFLMAP::iFunc

Index of 'function' (0 if none)

xU64 AFLMAP::nAdr

Code address.

UINT AFLMAP::nLine

Code line number.

int AFLMAP::nRes[5]

Reserved.

char AFLMAP::szFile[1]

Filename and function (0 [,'filename',0 [,'function',0]])