Using the µVision Socket Interface: Progressbar Command Codes

| Using the µVision Socket Interface Application Note 198 Control and monitor µVision via the built-in TCP/IP interface

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations
Progressbar Command Codes
Enumerations

## Enumerations
enum | PGCMD { UV_PROGRESS_INIT = 1, UV_PROGRESS_SETPOS = 2, UV_PROGRESS_CLOSE = 3, UV_PROGRESS_INITTXT = 4, UV_PROGRESS_SETTEXT = 5, UV_PROGRESS_END }

## Description

## Enumeration Type Documentation

enum PGCMD

uVision Progress bar control type definition

Indicates the type of uVision progress bar operation to perform.

Enumerator
UV_PROGRESS_INIT | Initialize progress bar with optional label (in %-mode)
UV_PROGRESS_SETPOS | Set progress bar percentage (0...100)
UV_PROGRESS_CLOSE | Close the progress bar.
UV_PROGRESS_INITTXT | Initialize progress bar (in text mode)
UV_PROGRESS_SETTEXT | Set inside bar text in text mode.
UV_PROGRESS_END | Always at end.